|  |  |  |
| --- | --- | --- |
|  |  |  |

**Motorové kondenzátory, SR Passives**

logo[[](https://www.tme.eu/html/gfx/image_16190.jpg)](https://www.tme.eu/html/gfx/image_16190.jpg)

|  |  |
| --- | --- |
| **Typ kondenzátora** | polypropylénový |
| **Prac. napätie** | 450 V |
| **Tolerancia** | ±5% |
| **Klimatická kategória** | 25/70/21 |
| **Životnosť** | 3000 h |
| **Pracovná teplota** | -25...70°C |
| |  |  |  | | --- | --- | --- | | **Symbol** | **Kap.** | **Rozm. tel.** | |  | **[µF]** | **[mm]** | | [**CBB60E-1/450**](https://www.tme.eu/sk/details/cbb60e-1_450/motorove-kondenzatory/sr-passives/) | 1 | Ø30x57 | | [**CBB60A-1.5/450**](https://www.tme.eu/sk/details/cbb60a-1.5_450/motorove-kondenzatory/sr-passives/) | 1,5 | Ø30x60 | | [**CBB60E-1.5/450**](https://www.tme.eu/sk/details/cbb60e-1.5_450/motorove-kondenzatory/sr-passives/) | 1,5 | Ø30x57 | | [**CBB60A-2/450**](https://www.tme.eu/sk/details/cbb60a-2_450/motorove-kondenzatory/sr-passives/) | 2 | Ø30x60 | | [**CBB60E-2/450**](https://www.tme.eu/sk/details/cbb60e-2_450/motorove-kondenzatory/sr-passives/) | 2 | Ø30x57 | | [**CBB60A-2.5/450**](https://www.tme.eu/sk/details/cbb60a-2.5_450/motorove-kondenzatory/sr-passives/) | 2,5 | Ø30x60 | | [**CBB60E-2.5/450**](https://www.tme.eu/sk/details/cbb60e-2.5_450/motorove-kondenzatory/sr-passives/) | 2,5 | Ø30x57 | | [**CBB60G-2.5/450**](https://www.tme.eu/sk/details/cbb60g-2.5_450/motorove-kondenzatory/sr-passives/) | 2,5 | Ø35x65 | | [**CBB60H-2.5/450**](https://www.tme.eu/sk/details/cbb60h-2.5_450/motorove-kondenzatory/sr-passives/) | 2,5 | Ø35x60 | | [**CBB60G-3/450**](https://www.tme.eu/sk/details/cbb60g-3_450/motorove-kondenzatory/sr-passives/) | 3 | Ø35x65 | | [**CBB60H-3/450**](https://www.tme.eu/sk/details/cbb60h-3_450/motorove-kondenzatory/sr-passives/) | 3 | Ø35x60 | | [**CBB60E-4/450**](https://www.tme.eu/sk/details/cbb60e-4_450/motorove-kondenzatory/sr-passives/) | 4 | Ø35x65 | | [**CBB60H-4/450**](https://www.tme.eu/sk/details/cbb60h-4_450/motorove-kondenzatory/sr-passives/) | 4 | Ø35x60 | | [**CBB60A-4.5/450**](https://www.tme.eu/sk/details/cbb60a-4.5_450/motorove-kondenzatory/sr-passives/) | 4,5 | Ø35x60 | | [**CBB60E-4.5/450**](https://www.tme.eu/sk/details/cbb60e-4.5_450/motorove-kondenzatory/sr-passives/) | 4,5 | Ø35x60 | | [**CBB60A-6/450**](https://www.tme.eu/sk/details/cbb60a-6_450/motorove-kondenzatory/sr-passives/) | 6 | Ø35x60 | | [**CBB60E-6/450**](https://www.tme.eu/sk/details/cbb60e-6_450/motorove-kondenzatory/sr-passives/) | 6 | Ø35x65 | | [**CBB60G-6/450**](https://www.tme.eu/sk/details/cbb60g-6_450/motorove-kondenzatory/sr-passives/) | 6 | Ø35x65 | | [**CBB60H-6/450**](https://www.tme.eu/sk/details/cbb60h-6_450/motorove-kondenzatory/sr-passives/) | 6 | Ø35x60 | | [**CBB60A-8/450**](https://www.tme.eu/sk/details/cbb60a-8_450/motorove-kondenzatory/sr-passives/) | 8 | Ø35x60 | | [**CBB60E-8/450**](https://www.tme.eu/sk/details/cbb60e-8_450/motorove-kondenzatory/sr-passives/) | 8 | Ø35x65 | | [**CBB60F-8/450**](https://www.tme.eu/sk/details/cbb60f-8_450/motorove-kondenzatory/sr-passives/) | 8 | Ø35x60 | | [**CBB60G-8/450**](https://www.tme.eu/sk/details/cbb60g-8_450/motorove-kondenzatory/sr-passives/) | 8 | Ø35x65 | | [**CBB60H-8/450**](https://www.tme.eu/sk/details/cbb60h-8_450/motorove-kondenzatory/sr-passives/) | 8 | Ø35x60 | | [**CBB60A-10/450**](https://www.tme.eu/sk/details/cbb60a-10_450/motorove-kondenzatory/sr-passives/) | 10 | Ø35x60 | | [**CBB60E-10/450**](https://www.tme.eu/sk/details/cbb60e-10_450/motorove-kondenzatory/sr-passives/) | 10 | Ø35x65 | | [**CBB60G-10/450**](https://www.tme.eu/sk/details/cbb60g-10_450/motorove-kondenzatory/sr-passives/) | 10 | Ø35x65 | | [**CBB60H-10/450**](https://www.tme.eu/sk/details/cbb60h-10_450/motorove-kondenzatory/sr-passives/) | 10 | Ø35x60 | | | | |  |  |  | | --- | --- | --- | | **Symbol** | **Kap.** | **Rozm. tel.** | |  | **[µF]** | **[mm]** | | [**CBB60A-12/450**](https://www.tme.eu/sk/details/cbb60a-12_450/motorove-kondenzatory/sr-passives/) | 12 | Ø40x70 | | [**CBB60E-12/450**](https://www.tme.eu/sk/details/cbb60e-12_450/motorove-kondenzatory/sr-passives/) | 12 | Ø40x70 | | [**CBB60A-14/450**](https://www.tme.eu/sk/details/cbb60a-14_450/motorove-kondenzatory/sr-passives/) | 14 | Ø40x70 | | [**CBB60E-14/450**](https://www.tme.eu/sk/details/cbb60e-14_450/motorove-kondenzatory/sr-passives/) | 14 | Ø40x70 | | [**CBB60H-14/450**](https://www.tme.eu/sk/details/cbb60h-14_450/motorove-kondenzatory/sr-passives/) | 14 | Ø42x70 | | [**CBB60A-16/450**](https://www.tme.eu/sk/details/cbb60a-16_450/motorove-kondenzatory/sr-passives/) | 16 | Ø40x70 | | [**CBB60E-16/450**](https://www.tme.eu/sk/details/cbb60e-16_450/motorove-kondenzatory/sr-passives/) | 16 | Ø40x70 | | [**CBB60G-16/450**](https://www.tme.eu/sk/details/cbb60g-16_450/motorove-kondenzatory/sr-passives/) | 16 | Ø40x70 | | [**CBB60H-16/450**](https://www.tme.eu/sk/details/cbb60h-16_450/motorove-kondenzatory/sr-passives/) | 16 | Ø42x70 | | [**CBB60A-20/450**](https://www.tme.eu/sk/details/cbb60a-20_450/motorove-kondenzatory/sr-passives/) | 20 | Ø40x70 | | [**CBB60E-20/450**](https://www.tme.eu/sk/details/cbb60e-20_450/motorove-kondenzatory/sr-passives/) | 20 | Ø40x70 | | [**CBB60G-20/450**](https://www.tme.eu/sk/details/cbb60g-20_450/motorove-kondenzatory/sr-passives/) | 20 | Ø40x70 | | [**CBB60H-20/450**](https://www.tme.eu/sk/details/cbb60h-20_450/motorove-kondenzatory/sr-passives/) | 20 | Ø40x70 | | [**CBB60E-25/450**](https://www.tme.eu/sk/details/cbb60e-25_450/motorove-kondenzatory/sr-passives/) | 25 | Ø42x95 | | [**CBB60G-25/450**](https://www.tme.eu/sk/details/cbb60g-25_450/motorove-kondenzatory/sr-passives/) | 25 | Ø45x95 | | [**CBB60H-25/450**](https://www.tme.eu/sk/details/cbb60h-25_450/motorove-kondenzatory/sr-passives/) | 25 | Ø42x82 | | [**CBB60A-30/450**](https://www.tme.eu/sk/details/cbb60a-30_450/motorove-kondenzatory/sr-passives/) | 30 | Ø45x90 | | [**CBB60E-30/450**](https://www.tme.eu/sk/details/cbb60e-30_450/motorove-kondenzatory/sr-passives/) | 30 | Ø45x90 | | [**CBB60G-30/450**](https://www.tme.eu/sk/details/cbb60g-30_450/motorove-kondenzatory/sr-passives/) | 30 | Ø45x95 | | [**CBB60H-30/450**](https://www.tme.eu/sk/details/cbb60h-30_450/motorove-kondenzatory/sr-passives/) | 30 | Ø50x90 | | [**CBB60A-40/450**](https://www.tme.eu/sk/details/cbb60a-40_450/motorove-kondenzatory/sr-passives/) | 40 | Ø48x93 | | [**CBB60E-40/450**](https://www.tme.eu/sk/details/cbb60e-40_450/motorove-kondenzatory/sr-passives/) | 40 | Ø50x106 | | [**CBB60A-50/450**](https://www.tme.eu/sk/details/cbb60a-50_450/motorove-kondenzatory/sr-passives/) | 50 | Ø50x106 | | [**CBB60E-50/450**](https://www.tme.eu/sk/details/cbb60e-50_450/motorove-kondenzatory/sr-passives/) | 50 | Ø50x106 | | [**CBB60A-60/450**](https://www.tme.eu/sk/details/cbb60a-60_450/motorove-kondenzatory/sr-passives/) | 60 | Ø50x106 | | [**CBB60E-60/450**](https://www.tme.eu/sk/details/cbb60e-60_450/motorove-kondenzatory/sr-passives/) | 60 | Ø50x106 | | [**CBB60A-80/450**](https://www.tme.eu/sk/details/cbb60a-80_450/motorove-kondenzatory/sr-passives/) | 80 | Ø58x120 | | [**CBB60E-80/450**](https://www.tme.eu/sk/details/cbb60e-80_450/motorove-kondenzatory/sr-passives/) | 80 | Ø60x120 | | [**CBB60E-100/450**](https://www.tme.eu/sk/details/cbb60e-100_450/motorove-kondenzatory/sr-passives/) | 100 | Ø60x120 | |

**Vývody**:

* konektory 6,3mm (**CBB60E-xxx/450**, **CBB60A-xxx/450**)
* očkové M4 (**CBB60G-xxx/450**, [**CBB60F-8/450**](https://www.tme.eu/sk/details/cbb60f-8_450/motorove-kondenzatory/sr-passives/))
* vodiče (**CBB60G-xxx/450**, **CBB60H-xxx/450**, [**CBB60F-8/450**](https://www.tme.eu/sk/details/cbb60f-8_450/motorove-kondenzatory/sr-passives/))

**Upevnenie** (**CBB60E-xxx/450**, **CBB60G-xxx/450**):

* skrutka M8

**Dĺžka kábla** ([**CBB60G-2.5/450**](https://www.tme.eu/sk/details/cbb60g-2.5_450/motorove-kondenzatory/sr-passives/), [**CBB60G-20/450**](https://www.tme.eu/sk/details/cbb60g-20_450/motorove-kondenzatory/sr-passives/), [**CBB60G-3/450**](https://www.tme.eu/sk/details/cbb60g-3_450/motorove-kondenzatory/sr-passives/), [**CBB60G-30/450**](https://www.tme.eu/sk/details/cbb60g-30_450/motorove-kondenzatory/sr-passives/), [**CBB60G-6/450**](https://www.tme.eu/sk/details/cbb60g-6_450/motorove-kondenzatory/sr-passives/), [**CBB60G-8/450**](https://www.tme.eu/sk/details/cbb60g-8_450/motorove-kondenzatory/sr-passives/), [**CBB60G-10/450**](https://www.tme.eu/sk/details/cbb60g-10_450/motorove-kondenzatory/sr-passives/), [**CBB60G-16/450**](https://www.tme.eu/sk/details/cbb60g-16_450/motorove-kondenzatory/sr-passives/), [**CBB60H-25/450**](https://www.tme.eu/sk/details/cbb60h-25_450/motorove-kondenzatory/sr-passives/)):

* 190 mm